#!/bin/sh
#
# UVify Core specific board defaults
#------------------------------------------------------------------------------


if [ $AUTOCNF = yes ]
then
	# Disable safety switch by default
	param set CBRK_IO_SAFETY 22027

	# don't probe external I2C
	param set SENS_EXT_I2C_PRB 0
fi
