#!/bin/sh
#
# @name Generic 10" Quad + geometry
#
# @type Quadrotor +
# @class Copter
#
# @output MAIN1 motor 1
# @output MAIN2 motor 2
# @output MAIN3 motor 3
# @output MAIN4 motor 4
# @output MAIN5 feed-through of RC AUX1 channel
# @output MAIN6 feed-through of RC AUX2 channel
#
# @output AUX1 feed-through of RC AUX1 channel
# @output AUX2 feed-through of RC AUX2 channel
# @output AUX3 feed-through of RC AUX3 channel
# @output AUX4 feed-through of RC FLAPS channel
#
# @maintainer Lorenz Meier <lorenz@px4.io>
#
# @board intel_aerofc-v1 exclude
# @board bitcraze_crazyflie exclude
#

. /etc/init.d/rc.mc_defaults

set MIXER quad_+

set PWM_OUT 1234
