#!/bin/sh
#
# mRo x21 specific board defaults
#------------------------------------------------------------------------------

# to minimize cpu usage on older boards limit inner loop to 400 Hz by default
if param compare IMU_GYRO_RATEMAX 0
then
	param set IMU_GYRO_RATEMAX 400
fi

if [ $AUTOCNF = yes ]
then

fi
