#!/bin/sh
#
# PX4 FMUv4 specific board defaults
#------------------------------------------------------------------------------


if [ $AUTOCNF = yes ]
then
	# Disable safety switch by default
	param set CBRK_IO_SAFETY 22027

fi

safety_button start

