#!/bin/sh
#
# @name FX-79 Buffalo Flying Wing
#
# @type Flying Wing
# @class Plane
#
# @output MAIN1 right aileron
# @output MAIN2 left aileron
# @output MAIN4 throttle
#
# @output AUX1 feed-through of RC AUX1 channel
# @output AUX2 feed-through of RC AUX2 channel
# @output AUX3 feed-through of RC AUX3 channel
#
# @maintainer Simon Wilks <simon@uaventure.com>
#
# @board px4_fmu-v2 exclude
# @board bitcraze_crazyflie exclude
#

. ${R}etc/init.d/rc.fw_defaults

param set-default FW_AIRSPD_MAX 30
param set-default FW_AIRSPD_MIN 13
param set-default FW_AIRSPD_TRIM 15

param set-default NAV_LOITER_RAD 150


set MIXER FX79
