#!/bin/sh
#
# PX4 FMUv5 specific board sensors init
#------------------------------------------------------------------------------

board_adc start

# Internal SPI bus ICM-20602
icm20602 -s -R 2 -q start

# Internal SPI bus ICM-20689
icm20689 -s -R 2 start

# Internal SPI bus BMI055 accel/gyro
bmi055 -A -R 2 -s start
bmi055 -G -R 2 -s start

# Baro on internal SPI
ms5611 -s start

# internal compass
ist8310 -I -R 10 start

# External compass on GPS1/I2C1 (the 3rd external bus): standard Holybro Pixhawk 4 or CUAV V5 GPS/compass puck (with lights, safety button, and buzzer)
ist8310 -X -b 1 -R 10 start
